**Interface Control Document (ICD)**

1. **Scope**

SEDAP-Express is an exceptionally fast path to integrate new applications, sensors, effectors or other similar things into the ecosystem of MESE. That's why it is intentionally kept simple and offers several technical ways of communication. Of course, this results in limitations, but in most cases where quick and easy integration is required, these are negligible. If increased demands arise later on, the “bigger” SEDAP API respective MESE interface can be used if necessary. SEDAP-Express is licensed under the “Simplified BSD License” (BSD-2-Clause). Therefore, there should be no problems using SEDAP-Express in commercial or non-commercial projects or integrating parts of the SEDAP-Express framework. Everything you need for development and testing can be found on the Internet at <https://SEDAP.Express>.

1. **Glossary**

MESE = Military Expandable Software Environment

SEDAP = Safety critical Environment for Data exchange And Process scheduling

CSV = Comma-Separated-Values

SEC = SEDAP-Express-Connector (Part of MESE)

SECMockUp = Simulation of the real SEC and a C2-like system including distributing and a simple log plus map  
MessageTool = Tool for manual generation of messages

SIDC = Symbol identification code (APP-6A/B/MIL-STD-2525B/C/STANAG 2019)

ASCII = American Standard Code for Information Interchange – in this context the ISO-8859-1 table is meant

BASE64 = Binary-to-text encoding scheme, which is using an alphabet of 64 characters

1. **General connection guidelines**
2. **Common conventions**

* Basic format is CSV using ‘;’ (0x3B) as separation character between two data fields, excess semicolons can be truncated
* Elements of list values are separated by ‘#’ (0x23), List values are marked with a ‘\*’ in the specification
* Message ends with a ‘\n’ (0x0A) as termination
* Mandatory fields/elements except the name are marked with (M)
* Maximum length of untyped or text fields is 256 bytes
* The messages are human-readable and using the ASCII-table
* Fields with (Binary)Data which possibly contains a special character (e.g. 0x0A, 0x23, 0x3B) has to be encoded with BASE64
* Unknown/Invalid values must not be transmitted, the respective field will be left empty
* Support for IPv4 and IPv6 (except for serial connection)
* SEC/SECMockUp/Applications can send and receive at any time
* Application shall send heartbeat message not more often than with 1Hz (+-100ms), but can vary if it is required
* SEC/SECMockUp answers heartbeat also with a heartbeat message (see chapter IV.2.12)

1. **Authentication**

* If authentication/encryption is required, it’s always preferred to use VPN connections instead
* Messages could be authenticated by fulfilling the MAC field using a shared password (see chapter IV.1.1)
* The password can either be defined in advance or exchanged using the Diffie-Hellman process and the KEYEXCHANGE message (see chapter IV.2.14). It’s recommended to authenticate even this message with a pre-shared password.
* For calculating the MAC you have to use the complete message incl. header and setting the MAC temporary to “0000”
* To save data, it is possible to limit the MAC to the first 4 bytes/32 bits while reducing security
* At minimum standards defined by FIPS 140-2 (Federal Information Processing Standard) have to be used  
  That means it is preferred to use:
  + 32Bit/256Bit HMAC in combination SHA256 (FIPS 198-1 / RFC 2104)
  + 32Bit/128Bit CMAC in combination AES128 (NIST SP 800-38B)
  + 32Bit/128Bit GMAC in combination AES128 (NIST SP 800-38D)
* It’s recommended to use MAC DBRG (Deterministic Random Bit Generator, NIST SP 800-90A/B)  
    
  *Sample (32Bit CMAC, Password:expressexpressex):* OWNUNIT;5E;0195236D151A;66A3;R;;089A01E7;53.32;8.11;0;5.5;21;22;;;FGS Bayern

1. **Encryption**

* Encryption is optional and as already wrote, if authentication/encryption is required, it’s preferred to use VPN instead
* At minimum standards defined by FIPS 140-2 (Federal Information Processing Standard) have to be used  
  That means it is preferred to use:
  + AES128/256 CFB/NoPadding (NIST SP 800-38A)
  + AES128/256 CTR/NoPadding (NIST SP 800-38A)
  + AES128/256 ECB/PKCS7Padding (NIST SP 800-38A)
  + XOR (Pseudo-encryption ONLY for testing/debugging purposes or for very light obfuscation)
* It’s recommended to use MAC DBRG (Deterministic Random Bit Generator, NIST SP 800-90A/B)
* Encrypted data must be BASE64 encoded - all incl. header (see chapter IV.1.1.1) have to be encoded
* If there is password given every message have to be encrypted – mixture of encrypted and plain message is not allowed

*Sample reference message:*  
OWNUNIT;5E;01952384BD8D;66A3;R;;;53.32;8.11;0;5.5;21;22;;;FGS Bayern;sfspclff-------

*Sample encrypted message (AES128, CFB, Password:expressexpressex):*UdlsDIB4oeKiuU4PXtV9qCPrrk10yPFg38Bakm7oGVOOC3siuczsyg37+Q9eiDE1Z0qyaXQl4puRGdB0mpb1Vf6cfhj7n7270Gv/VjW5Ol8IAFJh

1. **Compression**

* Compression is optional (has to be used BEFORE an optional encryption because of the high entropy!)
* Use the widely spreaded “deflate” for compression (only effective if the message size exceeds 140 characters due to the BASE64 encoding)
* Compressed data must be BASE64 encoded – all incl. header (see chapter IV.1.1.1) have to be compressed
* If the first bytes of a received message don’t match a message name, prove for compression

Sample reference message:

TEXT;D3;01952381E21B;324E;S;TRUE;;;;1;NONE;"This is an alert!"

Sample compressed message:

C3GNCLF2MbY2MLQ0NTK2MHQ1MnSyNjYycbUOtg4JCnW1BgJDaz9/P1drpZCMzGIFIErMU0jMSS0qUVQCAA==

1. **TCP Connection**

* Standard port 50000, but customizable
* SEC/SECMockUp can play server or client role
* One should use only one TCP connection for any kind of message and keep it open

1. **UDP-Connection**

* Standard port 50000, but customizable
* Support for Uni-, Broad- or Multicast mode
* Standard Multicast-Address is 228.2.19.80 resp. ff02:8:2:19:80::1
* Multiple messages per UDP-packet possible
* HEARTBEAT messages should be answered with UDP-Unicast if possible (see chapter IV.2.12)
* Is highly recommended to use the <number> and <acknowledgement> field in the header cause of possible packet lost

1. **Serial connection**

* Standard 115200-8-N-1, Full-Duplex is preferred, Half-Duplex and Simplex without acknowledge requests
* There are three modes available, depending on the use case:
  + Message never contains a \n (0x0A), therefore the message could be sent with an additional appended \n\n\n\n
  + Message contains one or more \n (0x0A), have to be BASE64-encoded and sent with an additional appended \n\n\n\n

1. **REST-API**

* Standard ports are HTTP 80 or HTTPS 443, but customizable
* Deflate or GZip compression should be supported

1. **Protocol Buffers**

* Ports and other TCP or UDP parameters are the same as descripted in chapter III.5 and III.6.

1. **Specifications of the data exchange**
2. **General specifications**
   1. **TCP-/UDP-/Serial connections**

On principle, messages have a CSV structure with a common header:

<Name>(M);<Number>;<Time>;<Sender>;<Classification>;<Acknowledgement>;<MAC>;<Content>

Everything except the name is basically optional. Certain messages require specific header elements, such as time or the sender.  
These exceptions are described in the chapter of the respective message. Hexadecimal numbers have no “0x”-prefix.

|  |  |
| --- | --- |
| <Name> | Defines the purpose of a message. Sometimes it’s so-called topic. |
| <Number> | This is a hexadecimal string representation of a 7-bit sequential number. Each type of message has its own counter that starts again with zero after reaching 127/7F. A reconnect does not resets the counters! The limitation to 7-bit or a max of 127 prevents problems with signed/unsigned byte formats. |
| <Time> | A hexadecimal string representation of a 64-bit Unix time stamp with milliseconds. |
| <Sender> | You can use freely selected textual identifiers, e.g. “OKRA”. This field won’t be changed, even if a message has been forwarded or relayed. This sender identification can be chosen by the participants themselves or permanently assigned by a responsible institution when preparing a specific use/network. If information of a sub-system has to be forwarded the sender identification should be the source of the original information, in that case of the sub-system. For instance, if central unit relays information of drones in a swarm. |
| <Classification> | Describes the classification or security level of the content. Possible values are P=public, U=unclassified, R=restricted, C=confidential, S=secret, T=top secret |
| <Acknowledgement> | TRUE=request an acknowledgement, FALSE/Nothing=No acknowledgement. An acknowledgement of a messages requires a specified message number (second field of this header)! |
| <MAC> | A 32/128/256-bit wide hash-based message authentication code for verification (see chapter III.2 for more) |
| <Content> | Content of the message, depending on the message purpose. |

* 1. **REST-API connection**

If the REST-API shall be used, it’s preferred to also use the provided JSON schema file and the generated code which either comes with the SEDAP-Express SDK or has been generated by yourself. You can find the schema and sample requests/answers in chapter IV.3 or on <http://sepap.express>.

* 1. **Protobuf connection**

At least it’s also possible to use Google™ protocol buffers to exchange the SEDAP-Express messages. You can find the schema in chapter IV.4 or on <http://sepap.express>. This allows you to generate your own code or use the existing code from the framework or the sample client.

1. **Message specifications**

This is the list of all so-far available messages and their structures and content including some samples. All units of measurement are generally given in SI-units, but there are deviations where this makes sense due to the usual range of values. In the following the used units will be given within square brackets for all message-descriptions. The altitude is the altitude above sea-level. A value of zero means exactly on ground, if the position is on land. Latitude and longitude are in decimal degrees, while positive values means north and east respective negative values south and west. Relative position values are defined this way, that the x-axis points to the east direction, y-axis points to the north and the z-axis is equal to the height above the unit. Speed and course are meant to be relative to ground. Course and heading have a range from zero to 359.999, are relative to geographic north (zero degree) and rotate clockwise. In general, all values are optional. mandatory parameters are marked with (M). In general, numerical values are rational numbers (floating point), unless otherwise defined. In the examples, fields are sometimes intentionally shortened because they would otherwise be too large. This is the case, for example, with the KEYECHANGE message.

* 1. **OWNUNIT**

*Description:* Positional, kinematic and identification data of the own (sent by the client) or host (sent by the SEC) unit/platform.  
If a client is sending this message, it will be converted to a contact and sent into the MESE network. If there is more than one “own unit”, the “Sender” field must be filled in to distinguish between the different units.

*Structure:*  
OWNUNIT;<Number>;<Time>;<Sender>(M?);<Classification>;<Acknowledgement>;<MAC>;  
<Latitude>[°](M);<Longitude>[°](M);<Altitude>[m];  
<Speed over ground>[m/s];<Course over ground>[°];  
<Heading>[°];<Roll>[°];<Pitch>[°];  
<Name>;<SIDC>

*Sample 1:* OWNUNIT;5E;0191C643A8AF;DRONEONE;R;;;53.32;8.11;0;5.5;21;22;;;FGS Bayern;SFSPCLFF-------

*Sample 2:* OWNUNIT;11;0191C643A8AF;22AA;U;FALSE;4389F10D;77.88;-10.12;5577.0;33.44;55.66;1.1;-2.2;3.3;Ownunit;SFGPIB----H----

* 1. **CONTACT**

*Description:* Positional, kinematic and identification data of a contact. For example, this message would be used by a sensor to report a contact it recognized. In return this message would be used to receive the tactical picture from the MESE network.

*Structure:*  
CONTACT;<Number>;<Time>;<Sender>;<Classification>;<Acknowledgement>;<MAC>;  
<ContactID>(M);<DeleteFlag>;<Latitude>[°](M);<Longitude>[°](M);<Altitude>[m];  
<relative X-Distance>[m];< relative Y-Distance>[m];<relative Z-Distance>[m];  
<Speed over ground>[m/s];<Course over ground>[°];  
<Heading>[°];<Roll>[°];<Pitch>[°];  
<width>[m];<length>[m];<height>[m];  
<Name>;<Source>;<SIDC>;<MMSI>;<ICAO>;<Image>;<Comment>

|  |  |  |
| --- | --- | --- |
| ContactID | ASCII | A positive identification unique number or free text id of the contact chosen by the sender of this message |
| DeleteFlag | TRUE | Contact has to be removed |
| FALSE | Contact is current |
| Name | ASCII | Name of the contact, maximum length 64 bytes |
| Source | ASCII | Available types (more than one available): R=Radar, A=AIS, I=IFF/ADS-B, S=Sonar, E=EW, O=Optical, Y=Synthetic, M=Manual |
|  |  |
| SIDC | SIDC | Identification code, could be written in lower or upper case |
| MMSI | MMSI | Maritime Mobile Service Identity |
| ICAO | ICAO | International Civil Aviation Organization |
| Image | BASE64 | Image data (JPG, PNG, TIF) encoded in BASE64, maximum length 8192 bytes |
| Comment | BASE64 | Free text to the contact, maximum length 2048 bytes |

*Sample 1:* CONTACT;5E;0191C643A8AF;83C5;R;;;100;FALSE;53.32;8.11;0;;;;120;275;;;;;;;FGS Bayern;AR;SFSPCLFF-------;;;;VXNlIENIMjI=

*Sample 2:* CONTACT;5F;0191C643A8AF;83C5;U;;;101;;36.32;12.11;2000;;;;44;;;;;;;;Unknown;O;;221333201;;;UG9zcyBOZXRoZXJsYW5kcw==  
*Sample 3:* CONTACT;60;0191C643A8AF;4371;S;TRUE;;102;TRUE;53.32;8.11

* 1. **EMISSION**

*Description:* Positional, attributes and identification data of an electro-magnetic, optical or acoustic emission.

*Structure:*EMISSON;<Number>;<Time>;<Sender>;<Classification>;<Acknowledgement>;<MAC>;  
<EmissionID>(M);<DeleteFlag>;<SensorLatitude>[°](M);<SensorLongitude>[°](M);<SensorAltitude>[m];  
<EmitterLatitude>[°];<EmitterLongitude>[°];<EmitterAltitude>[m];  
<Bearing>[°](M);<Frequencies[Hz]\*>;<Bandwidth[Hz]>;<Power[db(A)]>;<FreqAgility>;<PRFAgility>;  
<Function>;<SpotNumber>;<SIDC>;<Comment>

|  |  |  |
| --- | --- | --- |
| EmissionID | ASCII | A positive identification unique number or free text id of the emission chosen by the sender of this message. This number should also be unique in terms of contact numbers. |
| DeleteFlag | TRUE | Emission has to be removed |
| FALSE | Emission is current |
| FreqAgility | 00 | Stable Fixed |
|  | 01 | Agile |
|  | 02 | Periodic |
|  | 03 | Hopper |
|  | 04 | Batch Hopper |
|  | 05 | Unknown |
| PRFAgility | 00 | Fixed periodic |
|  | 01 | Staggered |
|  | 02 | Jittered |
|  | 03 | Wobbulated |
|  | 04 | Sliding |
|  | 05 | Dwell switch |
|  | 06 | Unknown PRF |
|  | 07 | CW |
| Function | 00 | Unknown |
|  | 01 | ESM Beacon/Transponder |
|  | 02 | ESM Navigation |
|  | 03 | ESM Voice Communication |
|  | 04 | ESM Data Communication |
|  | 05 | ESM Radar |
|  | 06 | ESM IFF/ADS-B |
|  | 07 | ESM Guidance |
|  | 08 | ESM Weapon |
|  | 09 | ESM Jammer |
|  | 0A | ESM Natural |
|  | 0B | ACOUSTIC Object |
|  | 0C | ACOUSTIC Submarine |
|  | 0D | ACOUSTIC Variable Depth Sonar |
|  | 0E | ACOUSTIC Array Sonar |
|  | 0F | ACOUSTIC Active Sonar |
|  | 10 | ACOUSTIC Torpedo Sonar |
|  | 11 | ACOUSTIC Sono Buoy |
|  | 12 | ACOUSTIC Decoy Signal |
|  | 13 | ACOUSTIC Hit Noise |
|  | 14 | ACOUSTIC Propeller Noise |
|  | 15 | ACOUSTIC Underwater Telephone |
|  | 16 | ACOUSTIC Communication |
|  | 17 | ACOUSTIC Noise |
|  | 18 | LASER Range Finder |
|  | 19 | LASER Designator |
|  | 1A | LASER Beam Rider |
|  | 1B | LASER Dazzler |
|  | 1C | LASER Lidar |
| SIDC | SIDC | Identification code |
| Comment | BASE64 | Free text to the emission, maximum length 2048 bytes |

*Sample 1:* EMISSION;5E;0195238E15AD;66A3;R;;;100;;53.32;8.11;0;;;;20;8725000#8735000;20000;3;0;2;6;5;10233;;SA-8

*Sample 2:* EMISSION;5F;0195238E25AD;66A3;R;;;101;;54.86;9.32;0;52.12;9.80;50;233;25725;4000;1,5;2;0;6;;sngpesr--------

* 1. **METEO**

*Description:* Metrological data of the environment.

*Structure:*  
METEO;<Number>;<Time>;<Sender>;<Classification>;<Acknowledgement>; <MAC>;  
<SpeedThroughWater>[m/s];<WaterSpeed>[m/s];<WaterDirection>[°];<WaterTemperature>[°C];<WaterDepth>[m];  
<AirTemperature>[°C];<DewPoint>[°C];<HumidityRel>[%];<Pressure>[hPa];<WindSpeed>[m/s];<WindDirection>[°];  
<Visibility>[km];<CloudHeight>[m];<CloudCover>[%]

*Sample:* METEO;AC;0195238E25AD;74BE;U;;;15.4;15.5;;;;10.2;72;20.3;;55;1005;25;;;2500;33

* 1. **TEXT**

*Description:* Human readable textual data. This could be an alert message, but also a simple text message for chatting. If the text possibly contains special characters (e.g. UTF-x, 0x0A, 0x23, … see chapter III.1), it has to be BASE64-encoded and the encoding indicator has to be set. If the coding indicator is not set, no coding is assumed.

*Structure:*

TEXT;<Number>;<Time>;<Sender>;<Classification>;<Acknowledgement>;<MAC>;<Recipient>;<Type>;<Encoding>;<Text>(M)

|  |  |  |
| --- | --- | --- |
| Recipient | ASCII | You can use a freely selected textual identifiers, as explained in the table from chapter IV.1.1. |
| Type | 00 | Undefined |
|  | 01 | Alert |
|  | 02 | Warning |
|  | 03 | Notice |
|  | 04 | Chat |
| Encoding | BASE64 | Text is BASE64 encoded |
|  | NONE | Text is not encoded |
| Text | ASCII | Free text of the message, maximum length 2048 bytes |
| Reference | ASCII | Reference to a contact or emission |

*Sample 1:* TEXT;D3;0195238E25AD;324E;S;TRUE;;;1;NONE;"This is an alert!";1000

*Sample 2:* TEXT;D4;0195238E25CC;324E;C;TRUE;;;2;NONE;"This is a warning!"

*Sample 3:* TEXT;D5;0195238E25EF;324E;R;;;;3;;"This is a notice!"

*Sample 4:* TEXT;D6;0195238E285B;324E;U;;;ORKA;4;BASE64;IlRoaXMgaXMgYSBjaGF0IG1lc3NhZ2UhIg==

* 1. **GRAPHIC**

*Description:* Define graphical plans likes polygons, squares or routes

*Structure:*  
GRAPHIC;<Number>;<Time>;<Sender>;<Classification>;<Acknowledgement>;<MAC>;  
<GraphicType>(M);<LineWidth>;<LineColor>;<Annotation>;<additional GraphicType-dependent parameters>\*

|  |  |  |
| --- | --- | --- |
| GraphicType | 00 | Point: <Latitude>[°];<Longitude>[°];<Altitude>[m] |
| 01 | Path: <Latitude>[°],<Longitude>[°],<Altitude>[m] # … |
|  | 02 | Polygon: <Latitude>[°],<Longitude>[°],<Altitude>[m] # … |
|  | 03 | Rectangle: <RotationAngle>[°];<Latitude1>[°],<Longitude1>[°],<Altitude1>[m]#<Latitude2>[°], <Longitude2>[°],<Altitude2>[m] |
|  | 04 | Square: <Latitude>[°];<Longitude>[°];<Altitude>[m];Radius-X[m];Radius-Y[m] |
|  | 05 | Circle: <Radius>[m];<Latitude>[°];<Longitude>[°];<Altitude>[m] |
|  | 06 | Ellipse: <Radius-X>[m];<Radius-Y>[m];<CenterLatitude>[°];<CenterLongitude>[°];<CenterAltitude>[m] |
|  | 07 | Block: <Latitude>[°];<Longitude>[°];<Altitude>[m];X-Radius [m];Y-Radius [m];Z-Radius [m] |
|  | 08 | Sphere: <Latitude>[°];<Longitude>[°];<Altitude>[m];Radius[m] |
|  | 09 | Ellipsoid: <Center\_Latitude>[°];<Center\_Longitude>[°];<Center\_Altitude>[m]; <Radius-X>[m];<Radius-Y>[m];<Radius-Z>[m] |
| LineWidth | => 1 | Width of the line or the point |
| LineColor | RGBA | Color of the line or the point in Web notation 800000FF for a darker red |
| FillColor | RGBA | Color of the line or the point in Web notation 00FF0080 for translucent green |
| Encoding | BASE64 | Text is BASE64 encoded |
|  | NONE | Text is not encoded |
| Annotation | ASCII | Text for an annotation to this graphic, maximum length 32 bytes |

*Sample 1:* GRAPHIC;79;0195238E35AD;910E;U;;;8;1;FF8000;BASE64;QXJlYSBBbHBoYQ==;10000;53.43;9.45

*Sample 2:* GRAPHIC;78;0195238E45AD;910E;U;;;1;1;808080;;Transit;54.23,12.86#54.30,12.9#54.55,13.3

* 1. **COMMAND**

*Description:* Command for one specific or all possible recipients. Which camera is assigned to which number and which camera modes are available must be defined specifically for each application and depending on the camera/sensor platform. The same also applies in particular for the generic action and any additional parameters for it. Time stamps are optional and in milliseconds. If no time stamp is given, it’s interpreted as instantly. Of course, you cannot use the generic SEDAP-Express connector in these cases, but must implement a specific and user-defined connector. Unix times stamps have to be written as hexadecimal string. Altitude is equivalent to depth.

*Structure:*

COMMAND;<Number>;<Time>;<Sender>;<Classification>;<Acknowledgement>;<MAC>;  
<Recipient>(M);<CmdID>;<CmdFlag>(M);<CmdType>(M);<additional cmdType-dependent parameters>\*

|  |  |  |
| --- | --- | --- |
| Recipient | ASCII | You can use a freely selected textual identifiers, as explained in the table from chapter IV.1.1. |
| CmdID | HexString | 16-Bit hexadecimal identifier of the command (0000 means all last commands) |
| CmdFlag | 00 | Add command |
|  | 01 | Replace (last) command |
|  | 02 | Cancel (last) command |
|  | 03 | Cancel all commands (Same as 02 if there it is not a command sequence) |
| CmdType | 00 | Power off: <Unix time stamp>;<Power on unix time stamp>(optional) |
|  | 01 | Restart: <Unix time stamp> |
|  | 02 | Standby: <Unix time stamp>;<Wakeup unix time stamp>(optional) |
|  | 03 | Sync time: <IP/Hostname of a NTP server> |
|  | 04 | Send status |
|  | 05 | Move: <Latitude>[°];<Longitude>[°];<Altitude>[m];<Tolerance>[m];<Unix time stamp> |
|  | 06 | Rotate: <HeadingAngle>[°];<RollAngle>[°];<PitchAngle>[°] |
|  | 07 | Loiter: <CenterLatitude>[°];<CenterLongitude>[°];<Altitude>[m];<Radius>[m] |
|  | 08 | Scan Area: <Latitude1>[°];<Longitude1>[°];<Latitude2>[°];<Longitude2>[°];<Altitude>[m];<Rotation>[°] |
|  | 09 | Take photo: <Number of camera>;<Camera mode> |
|  | 0A | Make video: <Number of camera>;<Camera mode>;<Duration> |
|  | 0B | Live video stream: <Number of camera>;<ON|OFF>;<Camera mode> (depends of the camera type) |
|  | 0C | <EngagementCmd[start-engagement|hold-engagement|stop-engagement]>;<WeaponID>;<ContactID> |
|  | EE | Sanitize system (e.g. in a case of emergency or drone hijacking) |
|  | FF | Generic Action: <Kind of action> (Has to be defined individually, inclusive implementing a custom connector software for MESE) |

*Sample 1:* COMMAND;55;0195238E25AD;5BCD;S;TRUE;4389F10D;ORKA;1111;01;0C;hold-engagement;bomb;1000  
*Sample 2:* COMMAND;29;0195238E35AD;E4B3;C;TRUE;;Drone1;;FF;00;OPEN\_BAY

*Sample 3:* COMMAND;29;0195238F55AD;E4B3;C;TRUE;;Drone2;0000;03 (Cancel all last commands)

*Sample 4: A complex move to with loitering at the end. The drone must calculate the speed itself based on the timestamp of the last move.*

COMMAND;29;0195238E25AD;E4B3;C;TRUE;;ORKA;0331;00;05;53.5143;8.1574;50;5

COMMAND;2A;0195238E25AD;E4B3;C;TRUE;;ORKA;0331;00;05;53.4897;8.1908;50;5

COMMAND;2B;0195238E25AD;E4B3;C;TRUE;;ORKA;0331;00;05;53.4694;8.2131;50;5

COMMAND;2C;0195238E25AD;E4B3;C;TRUE;;ORKA;0331;00;05;53.4397;8.2262;50;5;6644D570 (approx. 16 minutes later)

COMMAND;2D;0195238E25AD;E4B3;C;TRUE;;ORKA;0331;00;07;53.4397;8.2262;1000;200

* 1. **STATUS**

*Description:* This message transports some kinds of status variables like the remaining batterie capacity and optionally the execution status of the last or a specific command (see chapter IV.2.7). If the status information of a sub-system has to be forwarded, the sender identification should be the source of the original information, meaning for swarm of drones, the concrete, individual drone identification.

*Structure:*  
STATUS;<Number>;<Time>;<Sender>;<Classification>;<Acknowledgement>;<MAC>;  
<TecStatus>;<OpsStatus>;<AmmunitionLevel>\*;<FuelLevel>\*;<BatterieLevel>\*;<CmdID>;<CmdState>;<IP/Host>;<Media>\*;<Text>

|  |  |  |
| --- | --- | --- |
| TecStatus | 0 | Off/Absent |
|  | 1 | Initializing |
|  | 2 | Degraded |
|  | 3 | Operational |
|  | 4 | Fault |
| OpsStatus | 0 | Not operational |
|  | 1 | Degraded |
|  | 2 | Operational |
| AmmunitionLevel | String#% | Relative remaining ammunition: <name of the weapon>#<ammunition level>#.... |
| FuelLevel | String#% | Relative remaining fuel capacity: <name of the fuel tank>#<ammunition level>#.... |
| BatterieLevel | String#% | Relative remaining batterie capacity: <name of the batterie>#<batterie level>#.... |
| CmdID | HexString | ID of the related COMMAND message (16-bit) |
| CmdState | 00 | Undefined |
|  | 01 | Executed successfully |
|  | 02 | Partially executed successfully |
|  | 03 | Executed not successfully |
|  | 04 | Execution not possible (yet) |
|  | 05 | Will execute at ;<timestamp> |
| IP/Host | BASE64 | IP or hostname of the platform, maximum length 64 bytes |
| Media | BASE64 | List of video stream or image URLs, maximum length 4096 bytes |
| Text | BASE64 | Human readable free text description of the status |

*Sample 1:* STATUS;15;0195238E25AD;75DA;U;;;4;2;MLG#20;;Akku1#50;;;10.0.0.132;;RnVsbHkgb3BlcmF0aW9uYWw=

*Sample 2:* STATUS;16;0195238E25AD;129E;R;;;2;2;BMG#10;;;ED32;03;;aHR0cDovLzEwLjAuMC4xL2ltYWdlLnBuZw==;T3V0IG9mIGZ1ZWwh

* 1. **ACKNOWLEDGE**

*Description:* If a client or the SEC requested an acknowledge of a packet one has to use this this message. The acknowledgement flag is fixed set to FALSE. The awaiting client or SEC have to wait maximal one seconds before resending the original message with set acknowledgement flag.

*Structure:*

ACKNOWLEDGE;<Number>;<Time>;<Sender>;<Classification>;;<MAC>;  
<Recipient>(M);<Type of the message>(M);<Number of the message>(M)

|  |  |  |
| --- | --- | --- |
| Recipient | ASCII | You can use a freely selected textual identifiers, as explained in the table from chapter IV.1.1. |
| Type | ASCII | The type of the message which should be acknowledged (e.g. CONTACT, RESEND, …). |
| Number | HexString | The number of the message which should be acknowledged. This is a hexadecimal string representation of an 7-bit. |

*Sample:* ACKNOWLEDGE;18;0195238E25AD;129E;R;;;LASSY;COMMAND;2B

* 1. **RESEND**

*Description:* Missing messages can be requested again with this message. These messages can be recognized by the message number in the header, the sender ID and the message name as described in chapter IV.1.1.1.

*Structure:*

RESEND;<Number>;<Time>;<Sender>;<Classification>;<Acknowledgement>;<MAC>;  
<Recipient>(M);<Name of the missing message>(M);<Number of the missing message>(M)

|  |  |  |
| --- | --- | --- |
| Recipient | ASCII | You can use a freely selected textual identifiers, as explained in the table from chapter IV.1.1. |
| Name | ASCII | The name of the message which should resend. |
| Number | Number | The number of the message which should resend. This is a hexadecimal string representation of a 7-bit integer. |

*Sample:* RESEND;20;0195238E25AD;129E;R;;;FE2A;TEXT;5D

* 1. **GENERIC**

*Description:* This message is an empty container for transporting any kind of data. It has to be defined in the respective case. For example, one can use it to exchange the original MESE/SEDAP messages or other propriety protocol data. In the last case you have to use any other self-defined type. If the coding indicator is not set, no coding is assumed.

*Structure:*

GENERIC;<Number>;<Time>;<Sender>;<Classification>;<Acknowledgement>;<MAC>;

<ContentType>;<Encoding>;<Content>

|  |  |  |
| --- | --- | --- |
| ContentType | SEDAP | Content is an original MESE message |
| ASCII | Content is a custom-defined ASCII string |
|  | NMEA | Content is a NMEA0183 string |
|  | XML | Content is in an XML structure |
|  | JSON | Content is JSON formatted |
|  | BINARY | Self-defined binary array |
| Encoding | BASE64 | Content is BASE64 encoded |
| NONE | Content is NOT encoded |
| Content |  | Any content in printable ASCII or BASE64 encoded data, maximum length 8192 bytes |

*Sample 1:* GENERIC;5E;0195238E25AD;66A3;R;;;SEDAP;FALSE;

*Sample 2:* GENERIC;5E;0195238E25AD;66A3;R;TRUE;;SEDAP;TRUE;U2FtcGxlIGJpbmFyeSBkYXRhIEdyZWV0aW5ncyA6RA==

*Sample 3:* GENERIC;5E;0195238E25AD;66A3;R;;;NMEA;;$RATTM,11,11.4,13.6,T,7.0,20.0,T,0.0,0.0,N,,Q,,154125.82,A,\*17

* 1. **HEARTBEAT**

*Description:* This message offers the possibility to check the connection, which is primarily important, if you are using UDP or serial connection. It should not be sent more often than 1Hz. Nevertheless, if it is needed – one can use a faster repetition. The recipient field is optional and can be one single recipient or a list of more than one recipient. If no recipient is provided than all possible recipients in the network/serial net are addressed. A heartbeat message has an empty acknowledgement flag, because you cannot request one for it. Besides this, the acknowledgement flag is fixed set to FALSE (empty field).

*Structure:*  
HEARTBEAT;<Number>;<Time>;<Sender>;<Classification>;<Acknowledgement>;<MAC>;<Recipient>

|  |  |  |
| --- | --- | --- |
| Recipient | ASCII | You can use a freely selected textual identifiers, as explained in the table from chapter IV.1.1. |

*Sample 1:* HEARTBEAT;42;0195238E25AD;89AD;U;;;ORKA

*Sample 2:* HEARTBEAT;43;;1022

*Sample 3:* HEARTBEAT;43;

*Sample 4:* HEARTBEAT

* 1. **TIMESYNC**

*Description:* A correctly synchronized time often plays an important role. In general, you should use operating system functions/command line tools and a dedicated time server. But if this is not available for reasons, there is this message dedicated for this purpose. If necessary, a client should perform time synchronization himself from time to time.

If a TIMESYNC message is received, the current system time of the recipient must be included as timestamp in the response. The original sender can then calculate the round-trip time (RTT) from half the difference between the time the response was received and the time the message was sent and add it to the transmitted timestamp. The result can then be adopted as the new system time.

*Structure:*  
TIMESYNC;<Number>;<Time>;<Sender>;<Classification>;<Acknowledgement>;<MAC>;<Timestamp>

|  |  |  |
| --- | --- | --- |
| Timestamp | HexString | A hexadecimal string representation of a 64-bit Unix time stamp with milliseconds. |

*Sample 1:* TIMESYNC;42;0191C643A8AF;89AD;U

*Sample 2:* TIMESYNC;12;;FE2A;U;;;0191C643A8AF



* 1. **KEYEXCHANGE**

*Description:* If you don’t have the possibility to exchange a password/key via another channel (e.g., mail, telco), this message can be used to exchange keys via Diffie-Hellman-Merkle or via the post-quantum Kyber-/FrodoKEM process. It’s preferred to use ECDH or standard DH with MAC DRBG. If possible, also use MAC authentication for these messages or otherwise do some plausibility checks. The current phase defines if a field is mandatory. Both sides can restart the process by simply sending a message with the phase set again to zero again. The other side should restart the whole process inclusive generating new key pairs if using ECDH or Kyber-/FrodoKEM. Please pay attention, that the ECDH has no phase 1. The whole process always ends by sending a finalization confirmation.

To generate a 128- or 256-bit key from a larger secret key, “PBKDF2 with HMACSHA256” must be used with 1 iteration and no salt.

*Structure:*  
KEYEXCHANGE;<Number>;<Time>;<Sender>;<Classification>;<Acknowledgement>;<MAC>;<Recipient>;<AlgorithmType>(M);<Phase>(M); <KeyLengthSharedSecret>(M);<KeyLengthKEM>(M);<Prime>(M);<Natural number>(M);<InitialisationVector>(M);<Public variable\key>(M)

|  |  |  |
| --- | --- | --- |
| AlgorithmType | 0 | DH (Diffie-Hellman-Merkle 1024/2048 bit length, NIST SP 800-56A/B & 90A/B) |
|  | 1 | ECDH (Diffie-Hellman-Merkle with Curve25519 / X25519, 1024/2048/4096 bit length) |
|  | 2 | Kyber-512 |
|  | 3 | Kyber-768 |
|  | 4 | Kyber-1024 |
|  | 5 | FrodoKEM-640 (AES) |
|  | 6 | FrodoKEM-976 (AES) |
|  | 7 | FrodoKEM-1344 (AES) |
| Phase | 0,1,2 | Defines the current step in the key exchange process |
| KeyLengthSharedSecret | 128, 256 | Bit length of the shared secret key (Phase 0) |
| KeyLengthKEM | 1024, 2048, 4096 | Bit length of the key used for DH or KEM process (Phase 0) |
| Prime (p) | HexString | Publicly known prime number (> 3000 bits / 375 byte) (Phase 0, DH only) |
| Natural number (g) | HexString | Publicly known natural number smaller than p (Phase 0, DH only) |
| Initialisation vector (IV) | HexString | Initialisation vector (IV) used for AES CFB/CTR encryption |
| Public variable/key | BASE64 | The public variable/key of the sender |

*Sample 1:* KEYEXCHANGE;0;0191C643A8AF;89AD;U;;;FE2A;0;128;1024;7FFFFFFF;822460DE

*Sample 2:* KEYEXCHANGE;0;0191C643A8AF;FE2A;U;;;89AD;1;128;2048;;6E6026EFF9D9EBEB9D4A973CB5C287DBD77D75EDDD2

*DH-, ECDH and Kyber/FrodoKEM sequences:*

*:* 

1. **SEDAP-Express JSON-Schema**

The JSON schema was intentionally kept very simple. The JSON message contains only a list of one or more SEDAP-Express messages in their original (JSON-compatible) format. This means that the same message classes could be used for parsing and generating. With GET request the client can retrieve messages. On the other side with POST the client can send messages to the server. For simplicity there is only one endpoint at all. You can mix different messages in a single POST request. Updates for existing messages, e.g. contacts, can be sent to the server with POST or alternatively with PUT.

*Endpoint:*

http://<ip>:<port>/SEDAPEXPRESS

*Schema:*

{

"messages":[

{

"message":""

}

]

}

*Sample GET request:*

GET /SEDAPEXPRESS HTTP/1.1  
Host: sample.host  
Accept: application/json

*Sample GET answer:*

HTTP/1.1 200 OK

Content-Type: application/json

Content-Length: 380

{

"messages":[

{

"message":"CONTACT;60;0191C643A8AF;66A3;S;TRUE;102;TRUE;53.32;8.11"

"message":"METEO;AC;0191C643A8AF;74BE;U;;15.4;15.5;;;10.2;72;20.3;;55;1005;25;;;2500;33"

"message":"TEXT;D6;0191C643A8AF;324E;S;;3;"This is a chat message!";E4F1"

"message":"GRAPHIC;79;0191C643A8AF;910E;U;;8;1;FF8000;Area A;10000;53.43;9.45"

}

]

}

*Sample POST request:*

POST /SEDAPEXPRESS HTTP/1.1  
Host: sample.host  
Accept: application/json

{

"messages":[

{

"message":" OWNUNIT;5E;0191C643A8AF;66A3;R;TRUE;;42.32;-123.11;10000;50.23;297;;;33.3;-0.15;sfapmf---------"

"message":"TEXT;AE;0191C643A8AF;374E;S;;3;"This is a chat message!";E4F1"

}

]

}

*Sample POST answer:*

HTTP/1.1 200 OK

Content-Type: application/json

{"success":"true"}

1. **SEDAP-Express Protobuf-Definition**

The Google™ Protocol buffer definition is kept very simple, too. As with JSON messages, the same classes could be used to parse or generate the actual content.

*Definiton:*

syntax = "proto3";

message SomeMessage {

message Messages {

string message = 1;

}

repeated Messages messages = 1;

}

1. **Contact**

**Please report any issues, suggestions, additions or whatever you have in mind with SEDAP-Express via GitHub, by email or by phone.**

Federal Armed Forces of Germany

German Naval Support Command

c/o Commander (OF-4) Volker Voß

Wibbelhofstraße 3

26384 Wilhelmshaven

Germany

|  |  |
| --- | --- |
| GitHub: | [github.com/MESE-Core/SEDAP-Express](https://github.com/MESE-Core/SEDAP-Express) |
| Internet: | [linkedin.com/in/volker-voss](file:///C:\Projekte\VolkerVoss\SEDAP-Express\Documentation\linkedin.com\in\volker-voss) |
| E-Mail: | [mese@bundeswehr.org](mailto:mese@bundeswehr.org) |
| Tel.: | +49 4421 68 67290 |